**Green Laser Marking Machine**

Compared with traditional laser marking machine, it has low energy consumption and easy maintenance. Based on the large energy of 532nm laser, the selectivity of marking materials is much better.

Features:

1. Equipped with protective cover
2. Marking accuracy under 10μm
3. High electro-optic conversion efficiency
4. Good cooling performance, small size
5. Improves the passing rate of finished products effectively
6. Easy operation, stable performance
7. Long life, low energy consumption
8. Easy maintenance, cost saving

Application:

1. Electrical appliances
2. Communications
3. Precision instruments
4. Electronic components
5. Electrical industry
6. Integrated circuits
7. Hardware tools products,
8. Auto parts,
9. Plastic products
10. Crafts ornaments, etc.

|  |  |
| --- | --- |
| **Model** | **LSG7EI** |
| Average Output Power | ≥7W@30KHZ  |
| Wave Length | 532nm |
| Frequency | 1-100KHZ  |
| Marking Area | 110mm×110mm(Standard) |
| Min Linear Width | ≤0.01mm  |
| Max Linear Speed | ≤7000mm/s |
| Power Supply | AC220V±15%  50Hz |

http://en.hglaser.com/product/Nd-YVO4-Green-Laser-Marking-Machine.htm